{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Chamfer Calc","Sheet2","Sheet3"],"not_rendered":{"images":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Chamfer Calc","index":0,"n_rows":25,"n_cols":10,"rows_kept":25,"merged":[[0,0,0,10],[4,0,4,6],[8,7,8,9],[19,7,19,9]],"flags":["formulas_cached_only"]}
["Lathe Chamfer Calculation Helper"]
[]
["TNR","X axis ","Z axis","Chamf Len","Chamf Ang","X stk/clr","Z stk/clr"]
[0.0312,{"v":0.25,"d":"0.2500"},{"v":0,"d":"0.0000"},{"v":0.03,"d":"0.0300"},{"v":45,"d":"45.00"},{"v":0,"d":"0.0000"},{"v":0.05,"d":"0.0500"}]
["Instructions:  Fill in the blue variables. The rest will be calculated for you!"]
[{"$nulls":8},"x","z"]
[{"$nulls":7},"Start point",{"v":0.05344692629208114,"d":"0.0534"},{"v":0.05,"d":"0.0500"}]
[{"$nulls":7},"End point",{"v":0.25,"d":"0.2500"},{"v":-0.04827653685395943,"d":"-0.0483"}]
[{"$nulls":7},"Outside Diameters"]
[{"$nulls":7},"Diameter NC Code:","G00  X0.0534  Z0.0500"]
[{"$nulls":8},"G01  X0.2500  Z-0.0483"]
[]
[{"$nulls":7},"Radius NC Code:","G00  X0.0267  Z0.0500"]
[{"$nulls":8},"G01  X0.1250  Z-0.0483"]
[]
[]
[{"$nulls":8},"x","z"]
[{"$nulls":7},"Start point",{"v":0.44655307370791886,"d":"0.4466"},{"v":0.05,"d":"0.0500"}]
[{"$nulls":7},"End point",{"v":0.25,"d":"0.2500"},{"v":-0.04827653685395943,"d":"-0.0483"}]
[{"$nulls":7},"Inside Diameters"]
[{"$nulls":7},"Diameter NC Code:","G00  X0.4466  Z0.0500"]
[{"$nulls":8},"G01  X0.2500  Z-0.0483"]
[]
[{"$nulls":7},"Radius NC Code:","G00  X0.2233  Z0.0500"]
[{"$nulls":8},"G01  X0.1250  Z-0.0483"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}